**MBB S/N 004 incoming inspection**

* Slightly crooked parts flagged as process indicators. Side overhang is >0 but <25%.

C139, C295

* Silkscreen worn away at high points of copper pour neat C60
* Connections not shiny – appears to be flux residue.
* Capacitor polarities good?
* IC orientations good
* Diode polarities good?
* Drill alignment good

Install \_\_\_\_

Install \_\_\_\_

Install \_\_\_\_

Install \_\_\_\_

Clean board of flux residue \_\_\_\_\_\_