**MBB S/N 006 incoming inspection**

* Slightly crooked resistors flagged as process indicators. Side overhang is >0 but <25%.

R52

* U10 is crooked. Within spec?
* Connections not shiny – appears to be flux residue.
* Capacitor polarities good?
* IC orientations good
* Diode polarities good?
* Drill alignment good

Install \_\_\_\_

Install \_\_\_\_

Install \_\_\_\_

Install \_\_\_\_

Clean board of flux residue \_\_\_\_\_\_