**CPUB S/N 004 incoming inspection**

* Connections not shiny – appears to be flux residue.
* Capacitor polarities good?
* IC orientations good
* Diode polarities good?
* Drill alignment good

Install \_\_\_\_

Install \_\_\_\_

Install \_\_\_\_

Install \_\_\_\_

Clean board of flux residue \_\_\_\_\_\_